***Platinum Collection***

**SPECIFICATIONS FOR 12.3MM LAMINATE**

|  |  |
| --- | --- |
| SIZE | Length: 47-13/16” (1215).Thickness:15/32” (12mm) |
| QUANTITY PER BOX | 19.73 SQFT |
| CERTIFICATION | ISO 9001ISO 14001 |
| ABRASION | AC-3 Class 31 |
| CARB COMPLIANCE | Phase 2: 0.21 PPM(California Standard) |
| EDGE PROFILE | Four Side Pressed Edge |
| WARRANTY | Limited 30 Years Residential |
| FINISH | Very |
| RECOMMENDED USAGE | Residential |
| INSTALLATION | Unilin |
| Recommended Underlayment | 3mm EVA |
| Room Sound improvement with 3mm EVA | Approx 40% |