**SPECIFICATIONS FOR 8.3MM LAMINATE**

|  |  |
| --- | --- |
| **QUANTITY PER BOX** | **20.56 SQFT/ 1.9101SQM** |
| **PIECES PER BOX** | **8** |
| **DIMENSIONS** | **1212 x 197 x 8MM****(47.7 x 7.76 x 1.33)** |
| **CERTIFICATION** | **ISO 9001****ISO 14001** |
| **RATING** | **AC3/CLASS 31** |
| **WEIGHT**  | **15.2 kg/box** |
| **CARB COMPLIANCE** | **PHASE 1: 0.21 PPM****(CALIFORNIA STANDARD)** |